Cloud Server 1.0.1 for Windows

Quick Start
------------------------------
Launch CloudServer.exe by double clicking it's icon. It is a GUI based app and not meant to be run from the command line.

After launching CloudServer.exe, the console window will indicate whether the server started successfully or not. If not, there is most likely a port conflict with another application running on your computer. If this is the case, simply enter a new port number and press "Restart Server".

You should also choose the disk and program directories on your computer at this time. Programs files must currently have the suffix '.prg' to be picked up by the application. Each time you change either of the directories (via the Browse) button, the directories are scanned for files and the number of files found is displayed in the console. Any disks or programs uploaded from the Flyer will be stored in the appropriate directory as well.

The directories (and port selection) are saved automatically when quitting the application.

Once the server is up and running, its IP address and PORT will be displayed in the console. Set up a new cloud server configuration on your Flyer using these settings. Note that authentication is not currently performed so the username and password entries may be left blank.

Next, just make sure this cloud configuration is selected on the Flyer (using the button) and you should be ready to use it just as you would any other cloud server (such as commodoreonline.com).

If you have any issues, questions or suggestions for future updates, contact support@retroswitch.com.

Version History
------------------------------
1.0.0    2/9/2012
  - Initial Release.

1.0.1    2/19/2012
  - Directory scan for disks and programs now recursive.
  - Fixed bug when receiving multiple disks in a single upload package from Flyer.
  - Fixed unterminated disk listing returned to Flyer when downloading disk(s).
  - Fixed issue with some error messages not getting returned to the Flyer (for display on the LCD).

